ILYAD Wash TW

Indoor projector for wall washing purposes mounting equipped with a bicolor LED.
Asymmetrical distribution for a homogenous wall washing effect.

Equipped with a power supply enabling the light intensity adjustment as well as the mix of white lights by two on-board potentiometers or via Bluetooth or DALI.

Tilt 146°.
Azimuth 365°.
Several mounting possibilities: 3 circuits track adaptor, hook mounting, tieback mounting. Other mounting options on demand.
Adjustments and positions maintained by friction and locking screw.