**SYCLOP LP 18**

High lumen output and low energy consumption 18W framing projector.

Focusabe optical zoom, beam angle from 18° to 42°.

Tool free, quick-and-easy removal of the rotating optical zoom to convert it into a spotlight.

Framing by 4 quick-and-easy-positioning shutters.

Light Leaks free.

Tool free access to the lenses.

230 Volts direct power supply.

Several mounting possibilities: 3 circuits track adaptor, hook mounting, tieback mounting and wall mounting. (Other mounting options on demand)

Tilt angle 200° - azimuth 365°.

Holding positions by friction and locking screw. Handle free.

Integrated magnetic filter holder.

Integrated Gobo holder and filter holder.