**DELTALINE1R**

**Indoor high power monochromic LED linear fixture. Equipped with an adapor for 12V 1 circuit track. 12V remote power supply (reference to be chosen according to project).**

**Linear fixture equipped with an on board dimming potentiometer.  
Tilt angle on longitudinal axis: +/- 100°.**