**ILYAD W LP18**

**Indoor projector for wall washing purposes. Projector equipped with a high-power LED. Asymmetrical distribution for a homogenous wall washing effect.**

**Tilt 146°.
Azimuth 365°.
Several mounting possibilities : 3 circuits track adaptor, hook mounting, tieback mounting. Other mounting options on demand.
Handle free.
Adjustments and positions maintained by friction and locking screw.**