**SYCLOP LP 25 DMX**

**High lumen output and low energy consumption framing projector. Focusabe optical zoom, beam angle from 18° to 42°.  
Framing by 4 quick-and-easy-positioning shutters.  
Light Leaks free.**

**Tool free, quick-and-easy removal of the optical rotating barrel to convert it into a spotlight.  
Tilt angle 200° - azimuth 365°.  
Tool free access to the lenses. Holding positions by friction and locking screw. Handle free.**

**Dimming control by DMX 512 signal.  
RDM addressing or defined in the factory.  
Factory configurations :  
• 8 or 16 bits  
• Linear dimming curve / Smoothed Linear curve / Squared curve / Logarithmic curve  
• Start-up Power percentage without DMX signal.  
• Percentage or last value in case of loss of DMX signal.**

**Input signal by Data track adaptor or XLR 5 in/out RJ 45 In/Out.  
230 Volts power supply: 3 circuits track adaptor Global Pulse or Eutrac Data, or Powercon in/out for the hook mounting version.  
Integrated Gobo holder and magnetic filter holder.  
Hook mounting version: supplied with TRUE 1 power cable and plug 2P+E, length 1 meter.**