**LEXYS ZOOM**

**Focusable and dimmable spotlight, equipped with a high output Led.  
Focusable optical zoom, beam angle 15° to 50°. Holding positions by tightening the locking pin**

**Tilt angle 320°.  
Azimuth 365° for tieback mounting version,  
Azimuth 350° for 3-circuits track adaptor mounting version (365° option available).  
Accessories: barndoors, filter holder, anti-glare louvre, snoot and half snoot.  
Dimmable by on-board potentiometer, Casambi, DALI 2, phase-cut.**