**MICROCAD 12V**

**Indoor Micro-framing projector.
Fitted with a 12V 1 circuit track adaptor. Framing by 4 shutters.
Tilt angle: 100°.
Azimuth : 350°.
Rotatable optical head (360°).**