**DELTALINE1**

**Monochrome indoor linear high output LED fixture. Supplied with 3 meters of cable.
Mounting by lateral mounting flanges (see available accessories).**

**End to end installation ensuring continuity and consistency of the lighting on its entire length. Tilt on longitudinal axis: +/- 180 °
Remote power supply (to be selected according to the project).**