ILYAD FRESNEL TW

Projector equipped with a fixed Fresnel optical lens and a bicolor LED.  
Suitable to achieve large, plain and homogeneous light effects, hot spot free.

Equipped with a power supply enabling the light intensity adjustment as well as the mix of white lights by two on-board potentiometers or via Bluetooth or DALI. Tilt 200°.  
Azimuth 365°.  
Several mounting possibilities: 3 circuits track adaptor, hook mounting, tieback mounting. Other mounting options on demand.  
Adjustments and positions maintained by friction and locking screw.